LOADING DOCK EQUIPMENT

PART  1	  GENERAL
1.1 		SECTION INCLUDES
A.		Loading dock equipment of the following types: 
1.		Control stations.
1.2 		RELATED SECTIONS
A.		Section 03100 - Concrete Forms and Accessories: Placement of anchors into concrete.
B.		Section 03300 -  Cast-In-Place Concrete: Docks and pits.
C.		Section 05500 -  Metal Fabrications: Metal angles for edge of dock.
1.3 		REFERENCES
A.		American National Standards Institute (ANSI):
1.		ANSI MH30.1-  Industrial Loading Dock Boards (Ramps).
2.		ANSI MH29.1-  Industrial Scissor Lifts.
3.	     ANSI MH30.3- Vehicle Restraining Devices (Safety, Performance, and Testing)
1.4 		SUBMITTALS
A.		Section 01330 -  Submittals Procedures: Procedures for submittals.
B.		Product Data:  For each product specified.
1.		Bumpers: Indicate unit dimensions, method of anchorage, and details of construction.
2.		Levelers: Indicate materials and finish, installation details, roughing-in measurements, and operation of unit.
C.		Shop Drawings:
1.		Indicate required opening dimensions, tolerances of opening dimensions, placement dimensions, and perimeter conditions of construction.
2.		Wiring diagrams including location of control stations and disconnect switches.
D.		Assurance/Control Submittals:
1.		Certificates: Manufacturer's certificate that Products meet or exceed specified requirements.
2.		Qualification Documentation: Submit documentation of experience indicating compliance with specified qualification requirements.
1.5 		QUALITY ASSURANCE
A.		Dock Levelers: Conform to requirements of ANSI MH30.1.
B.		Vehicle Restraining Devices: Conform to requirements of ANSI MH30.3.
C.		Manufacturer Qualifications:
1.		Manufacturer specializing in manufacturing Products specified with minimum 30 years’ experience.
2.		Manufacturer to have quality assurance improvement programs.
3.		Manufacturer shall be associated with Loading Dock Equipment Manufacturers (LODEM) setting ANSI standards.
4.		Manufacturers welding procedure compliant with A.W.S.D1 .1 specifications.
D.		Installer Qualifications:  Company specializing in performing the Work of this Section with minimum 5 years’ experience.
1.6 		DELIVERY, STORAGE, AND HANDLING
A.		Refer to Section 01600 - Product Requirements: Transporting, handling, storage, installation and protection of products.
1.7 		WARRANTY
A.		Warranty: Provide manufacturer's standard warranty.
PART  2	  PRODUCTS
2.1 		MANUFACTURERS
	Acceptable Manufacturer:  Blue Giant Equipment Corporation, which is located at:  410 Admiral Blvd.; Mississauga, ON, Canada L5T 2N6; Toll Free Tel: 800-872-2583; Tel: 905-457-3900; Fax: 905-457-2313; Email:  marketing@bluegiant.com; Web:  https://www.bluegiant.com
2.2 		DOCK CONTROL PANELS 
A.		Single Push Button Control Stations:  SP1 as manufactured by BLUE GIANT. 

1.		Type:  Model SP1; single push button control station.

2.		Function:  The SP1 controls an independent hydraulic dock leveler via a constant-pressure “I” (UP) button.

3.		Power:  __ V, __ Amps, __ Phase. 

4.		Construction and Finish:  NEMA4X/IP65 (wet and corrosion resistant) rated plastic enclosure. Overall dimensions 6-1/2 inch L x 3 -1/4 inch W x 5-1/8 inch D (165 x 83 x 130 mm).

5.		Warranty:  Warranties are subject to standard limitations on liability. Consult manufacturer for full details on warranty information and product registration. 

6.		Standard Features:  
a.		NEMA4X / IP65 polycarbonate enclosure- resistant to both corrosion and wet conditions. 
b.		UL/CE approved. 

END OF SECTION